# openMSX Console Command Reference

1. Introduction
2. Commands
   1. after
   2. bind / unbind / bind_default / unbind_default
   3. cart / cart<x>
   4. cassetteplayer
   5. cd<x>
   6. cycle / cycle_back
   7. debug
   8. disk<x> / virtual_drive
   9. diskmanipulator
   10. escape_grab
   11. exit
   12. ext
   13. filepool
   14. findcheat
   15. hd<x>
   16. help
   17. incr
   18. iomap
   19. keymatrixdown / keymatrixup
   20. laserdiscplayer
   21. list_extensions
   22. load_icons
   23. load_settings
   24. machine
   25. create_machine / load_machine / activate_machine / list_machines / delete_machine
   26. machine_info
   27. monitor_type
   28. mute_channels / unmute_channels / solo
   29. nowind<x>
   30. openmsx_info
   31. openmsx_update
   32. osd
   33. palette
   34. plug / unplug
   35. psg_profile
   36. record
   37. record_channels
   38. remove_extension
   39. reset
   40. reverse
   41. save_settings
   42. savestate / loadstate / list_savestates / delete_savestate
   43. screenshot
   44. set
   45. slotmap
   46. slotselect
   47. soundlog
   48. store_machine / restore_machine
   49. test_machine
   50. toggle
   51. trainer
   52. type
   53. unset
   54. user_setting
   55. vdpregs
   56. other
3. Old Commands
   1. alias / unalias
   2. decr
   3. quit
   4. restoredefault
4. Settings
   1. accuracy
   2. audio-inputfilename
   3. autoruncassettes
   4. autorunlaserdisc
   5. auto_enable_reverse
   6. blur
   7. bootsector
   8. brightness
   9. cmdtiming
   10. color_matrix
   11. console
   12. consolebackground
   13. consolecolumns
   14. consolefont
   15. consolefontsize
   16. console_history_size
   17. consoleplacement
   18. consolerows
   19. console_remove_doubles
   20. contrast
   21. cputrace
   22. debugoutput
   23. default_machine
   24. deinterlace
   25. DirAsDSKmode
   26. disablesprites
   27. display_deform
   28. enable_session_management
   29. frequency
   30. firmwareswitch
   31. fullscreen
   32. fullspeedwhenloading
   33. gamma
   34. glow
   35. grabinput
   36. horizontal_stretch
   37. inputdelay
   38. kbd_auto_toggle_code_kana_lock
   39. kbd_code_kana_host_key
   40. kbd_mapping_mode
   41. kbd_numkeypad_always_enabled
   42. kbd_numkeypad_enter_key
   43. kbd_trace_key_presses
   44. keyjoystick<n>.<button>
   45. led_<name>
   46. limitsprites
   47. master_volume
   48. maxframeskip
   49. midi-in-readfilename
   50. midi-out-logfilename
   51. minframeskip
   52. mode
   53. mute
   54. noise
   55. pause
   56. pause_on_lost_focus
   57. pointer_hide_delay
   58. power
   59. printerlogfilename
   60. print-resolution
   61. r800_freq / r800_freq_locked
   62. renderer
   63. renshaturbo
   64. resampler
   65. rs232-inputfilename
   66. rs232-outputfilename
   67. rtcmode
   68. samples
   69. save_settings_on_exit
   70. scale_algorithm
   71. scale_factor
   72. scanline
   73. sound_driver
   74. speed
   75. <soundchip>_balance
   76. <soundchip>_ch<channel>_record
   77. <soundchip>_ch<channel>_mute
   78. <soundchip>_detune_frequency
   79. <soundchip>_detune_percent
   80. <soundchip>_vibrato_frequency
   81. <soundchip>_vibrato_percent
   82. <soundchip>_volume
   83. throttle
   84. turborpause
   85. umr_callback
   86. vdpcmdinprogress_callback
   87. vdpcmdtrace
   88. videosource
   89. v9990cmdtrace
   90. z80_freq / z80_freq_locked

## Introduction

This manual describes all commands and settings which are available in openMSX. You can use them to control openMSX fully from the Console (a built in command line interface, use F10 to call it), via Tcl scripts and via remote connections (explained in Controlling openMSX from External Applications). If you want to unleash the full potential of openMSX or just want a reference of all available possibilities, this manual should serve you well.

## Commands

### after

Execute a command after a certain event occurs, for example a given amount of time has passed or the emulator has been idle for a given amount of time. Every postponed command executes just once; if you want a command to run periodically, you have to issue it again every time it runs. The `after` command returns the id of the postponed command. It is possible to query a list of postponed commands and also to cancel postponed commands.

usage:

`after time <seconds> <command>` | Execute a command after some time. Timescale is in MSX seconds.
`after realtime <seconds> <command>` | Execute a command after some time. Timescale is in host seconds.
`after idle <seconds> <command>` | Execute a command after some time being idle
`after frame <command>` | Execute a command when a video frame is finished (VDP scanning reaches vsync)
`after break <command>` | Execute a command after a breakpoint is reached
`after boot <command>` | Execute a command after a (re)boot
`after machine_switch <command>` | Execute a command after switch to new a machine
`after <input-event> <command>` | Execute a command after the given input event occurs. The events are e.g. mouse, joystick, focus and resize events, the same ones as for the bind command.
`after info` | List all postponed commands
`after cancel <id>` | Cancel the postponed command with given id

examples:
`after time 2.6 "set renderer SDLGL-PP"`
`after idle 100 exit`
`after info`
`after cancel after#2`
`after "mouse button1 down" foo`

### bind / unbind / bind_default / unbind_default

Associate events (such as key presses) with commands. Whenever the specified event occurs (e.g. you press the specified key), the corresponding command will be executed. Any Tcl command or combination of commands separated with `;` (normal Tcl syntax) can be used. To customize your bindings you should use the (un)bind commands. A script that wants to provide a default binding for its functionality needs to use `bind_default`. Using the `-repeat` option makes sure that if the event is repeated (especially useful for key events, so when keeping a key pressed), the command is repeated as well.

Events can be:

`<key>[,release]` | Short for `keyb <key>[,release]`
`keyb <key>[,release]` | <key> is pressed [or released]
`mouse button<n> <up/down>` | Mouse button <n> went up or down
`mouse motion <x> <y>` | Mouse motion of <x> and <y>
`joy<n> button<m> <up/down>` | Button <m> of joystick <n> went up/down
`joy<n> axis<m> <value>` | Axis <m> of joystick <n> got value <value>
`focus <boolean>` | The openMSX window got (1) or lost (0) focus

usage:

`bind` | Show all bindings
`bind <key>` | Show binding for the given key
`bind <event>` | Show binding for this event
`bind <event> [-repeat] <command>` | Make a new binding
`unbind <key>` | Undo binding for this event

examples:
`bind PAGEUP "set speed 100"`
`bind PAGEDOWN "set speed 50"`
Only run with full throttle while F9 is pressed (like BrMSX):
`unbind F9`
`bind F9 "set throttle off"`
`bind F9,release "set throttle on"`
Pause when window loses focus (like fMSX):
`bind "focus 0" "set pause on"`
`bind "focus 1" "set pause off"`
Middle-click to toggle input grabbing:
`bind "mouse button2 down" "toggle grabinput"`
Map button 8 of joystick 1 to F2-key:
`bind "joy1 button8 down" "keymatrixdown 6 0x40"`
`bind "joy1 button8 up" "keymatrixup 6 0x40"`
Use PageUp/Down to increase/decrease emulation speed.
`bind PAGEUP -repeat "incr speed 1"`
`bind PAGEDOWN -repeat "incr speed -1"`
Toggle fullscreen with ALT and ENTER.
`bind ALT+RETURN toggle fullscreen`

### cart / cart<x>

Insert a ROM cartridge in a running MSX. The `cart` command inserts the cartridge in the first available slot. The `carta`, `cartb` etc. commands insert it in the specified slot. The cartridges can be removed again with the `eject` subcommand.

ROM cartridges are a special class of extensions. For extensions that are not ROM cartridges, see the commands `ext`, `list_extensions` and `remove_extension`.

usage:

`cart KMARE.ROM` | Insert ROM cartridge in first free slot
`cart insert KMARE.ROM` | Insert ROM cartridge in first free slot
`carta USAS.ROM -ips USAS.IPS` | Insert ROM cartridge in slot A, with IPS patch applied to the ROM contents
`cartb NEMESIS.ROM -romtype Konami` | Insert ROM cartridge in slot B, and explicitly specify the mapper type (is normally auto detected)
`carta eject` | Eject the currently inserted cartridge from slot A

### cassetteplayer

Controls the openMSX cassette player. The various subcommands can be used to insert, remove, create and rewind tape images.

usage:

`cassetteplayer insert <tape image>` | Insert tape image (WAV or CAS format) in the cassette player
`cassetteplayer eject` | Remove tape from virtual cassette player
`cassetteplayer rewind` | Rewind the current tape
`cassetteplayer motorcontrol on|off` | Selects whether motor control signal (remote) is obeyed (default: on)
`cassetteplayer new [<tape image>]` | Create new tape image and go to record mode
`cassetteplayer play` | Go to play mode (when in record mode) and rewind the tape

### cd<x>

Change the CDROM image. The commands `cda`, `cdb` etc. are assigned to all available CDROM drives in the MSX. They will not correspond to drive names as used in MSX-DOS.

usage:

`cda <iso image>` | Use ISO image for CDROM drive "cda"
`cda insert <iso image>` | Use ISO image for CDROM drive "cda"
`cda eject` | Eject CDROM from CDROM drive "cda"
`cda` | Show current ISO image for CDROM drive "cda"

### cycle / cycle_back

Iterates through the values of an enumerated setting.

`cycle_back` does the same as `cycle`, but it goes in the opposite direction.

usage:

`cycle <setting>` | Changes the specified setting to the next value in the cycle
`cycle_back <setting>` | Changes the specified setting to the previous value in the cycle

examples:
`cycle scale_algorithm`
`cycle videosource`

### debug

This command provides access to the debugger functionality of openMSX. It's meant to be used by an external debugger (see also Controlling openMSX from External Applications). The general format of the debug command is:

`debug <subcommand> [<extra arguments>]`

where 'extra arguments' are specific for each subcommand. Below is a list of all subcommands:

`debug list` | Return a list of all debuggables. A debuggable is (part of) the state of a MSX device that can be accessed via these debug commands. Examples are: the VDP registers the currently visible memory for the Z80 the contents of the RAM
`debug desc <name>` | Return a description of this debuggable
`debug size <name>` | Return the size of this debuggable
`debug read <name> <addr>` | Read a byte from a debuggable
`debug write <name> <addr> <val>` | Write a byte to a debuggable
`debug read_block <name> <addr> <size>` | Read a whole block at once
`debug write_block <name> <addr> <values>` | Write a whole block at once
`debug probe <subcommand>` | See below.
`debug break` | Break CPU at current position
`debug breaked` | Query CPU break status
`debug cont` | Continue execution after break
`debug step` | Execute one instruction
`debug list_bp` | List the active breakpoints
`debug set_bp <addr> [<cond>] [<cmd>]` | Insert a new breakpoint at the given address. Optionally you can specify a condition and a command. When the CPU is about to execute the instruction at the given address, the condition will be evaluated, if this evaluates to true then the command is executed. The condition can be any Tcl expression and the command can be any Tcl command. The default condition is 'true' and the default command is `"debug break"`.
`debug remove_bp <id>` | Remove a certain breakpoint
`debug list_watchpoints` | List all defined watchpoints
`debug set_watchpoint <type> <region> [<cond>] [<cmd>]` | Insert a new watchpoint. When the CPU is about to read or write to/from the specified memory or I/O region, the condition is evaluated. If the condition evaluated to true, the command is executed. The condition and the command are similar to the ones in the `set_bp` subcommand. A watchpoint can either be set on a single memory address or I/O port (specify a single value), or on a whole memory or I/O port range (specify a begin/end pair). For example: `debug set_watchpoint write_mem {0x8000 0x8FFF}`
`debug remove_watchpoint <id>` | Remove a certain watchpoint
`debug list_conditions` | List the active conditions
`debug set_condition <cond> [<cmd>]` | Set a new debugger condition. Conditions are like breakpoints, but not tied to a specific address. Simulation is much slower when conditions are used (though generally while debugging this is not a problem).
`debug remove_condition <id>` | Remove a certain condition
`debug disasm [<addr>]` | Disassemble instructions at PC or given address

The probe subcommand again has subcommands:

`debug probe list` | Returns a list of all probes.
`debug probe desc <probe>` | Returns a description of this probe.
`debug probe read <probe>` | Returns the current value of a probe. But note that not all probes have a value
`debug probe set_bp <probe> [<cond>] [<cmd>]` | Set a breakpoint of a probe. Like in the 'set_bp' subcommand you can optionally specify a condition and a command.
`debug probe remove_bp <id>` | Remove the given breakpoint.
`debug probe list_bp` | List the active breakpoints set on probes.

At first sight 'probes' and 'debuggables' are very similar. Though there are some important differences and that's why probes and debuggables use different subcommands:

A debuggable is an array of bytes. | A probe is a single value and can have any type.
A debuggable is readable and (usually) writable. | A probe is always read-only.
It's not possible to set breakpoints on a debuggable. | You can set breakpoints on a probe (and sometimes this is the only purpose of a probe).

Many examples of usage of the debug command can be found in the scripts that come with openMSX (in the `share/scripts` directory). We also list a few here.

examples:

- break (only!) after 0 is written to 0x8000):
  `debug set_watchpoint write_mem 0x8000 {[debug read "memory" 0x8000] == 0x00}`
- break on address 0xF37D, but only when Z80 register C has the value 0x2F:
  `debug set_bp 0xF37D {[reg C] == 0x2F}`
- break when CPU reads from any addresses between 0xFBE5 and 0xFBEF:
  `debug set_watchpoint read_mem {0xFBE5 0xFBEF}`
- break after a write was done to I/O port 0x99, but only when Z80 register A has a value of 0x81:
  `debug set_watchpoint write_io 0x99 {[reg A] == 0x81}`
- break as soon as there is a pending Z80 IRQ (even when in DI mode):
  `debug probe set_bp z80.pendingIRQ`
- break when register HL has the value 1234:
  `debug set_condition {[reg hl] == 1234}`

Note: Some of the commands are pretty low level. In the share/scripts directory you'll find some Tcl scripts that offer convenience wrappers around these commands. For example: `showmem`, `disasm`, `cpuregs`, `save_debuggable`, etc.

### disk<x> / virtual_drive

Insert a disk image in a drive. Optionally apply an IPS patch to the disk image. The commands `diska`, `diskb` etc. are assigned to all available "physical" disk drives in the MSX. They might not correspond to drive names as used in MSX-DOS.

In addition to the physical `disk<x>` drives, there is the `virtual_drive`. This fake drive does not correspond to any MSX hardware. It can be used as a source or target for `diskmanipulator` operations just like physical drives.

usage:

`diska <disk image>` | Insert disk image in drive "diska"
`diskb insert <disk image>` | Insert disk image in drive "diskb"
`diska <disk image> <ips>` | Insert disk image and apply IPS patch
`diska eject` | Remove disk from drive "diska"
`diska ramdsk` | Insert scratch disk in drive "diska"

### diskmanipulator

A collection of commands to manipulate (the files on) a disk image.

It can be used in so many different ways, that we wrote a separate manual for it: Using Diskmanipulator.

### escape_grab

Only has effect in windowed mode and when the `grabinput` setting is active. Temporarily release the input grab. After the openMSX window has lost and regained the focus, the grab is again effective.

usage:

`escape_grab` | Temporarily release the input grab

### exit

This command exits the Tcl interpreter, which leads to openMSX exiting as well.

usage:

`exit` | Exits the emulator

### ext

Insert an MSX extension in a running MSX machine. The extension can be removed again with the `remove_extension` command. See also the commands `cart`, `list_extensions` and `remove_extension`.

usage:

`ext fmpac` | Insert an FMPAC in a running MSX machine

### filepool

With this command you can manage your file pool settings. File pools are directories on your host system (PC/Mac/Dingoo/etc.). They are used by openMSX to search files in, which are referred to from machine or extension definition files, save states or replays which you are trying to load. First, the file will be searched at the path that was also used when the save state or replay was created. But if it isn't found there (which is usually the case if you load such a state or replay you got from someone else), it will use the file pools to search instead. In other words, if you are trying to load such replays, it's probably a good idea to put the media files referred to (ROMs, disks, tapes) in the (proper) filepool.

File pools have the following properties:

path
  The path to the directory which is the actual file pool
position
  There exists a list of file pools, which are searched in order of their position.
type(s)
  A file pool can serve specific types. Currently, the valid types are `system_rom` (for system ROMs, you are probably using this one already if you installed your system ROMs in the recommended place, `share/systemroms`), `rom` (for other ROM files), `disk` (for disk images) and `tape` for cassette/tape images.

Apart from the default sytem ROM file pool as mentioned above, the other default file pool is `share/software`, where openMSX will search for other (than system ROM) software.

usage:

`filepool list` | Shows the currently defined file pool entries (see below for example output)
`filepool add -path <path> -types <typelist> [-position <pos>]` | Add a new entry with the given properties as explained above. For the types, use a format like `"rom tape disk"`. Optionally, you can also specify where in the list of existing file pools the new file pool should be added. By default, this is at the end.
`filepool remove <position>` | Remove the file pool at the given position
`filepool reset` | Reset the file pool settings to the default values

An example of the default file pools for a Windows 7 system with user Quibus:

    1: C:/Users/Quibus/Documents/openMSX/share/systemroms  [system_rom]
    2: C:/Users/Quibus/Documents/openMSX/share/software  [rom disk tape]
    3: C:/Program Files/openMSX/share/systemroms  [system_rom]
    4: C:/Program Files/openMSX/share/software  [rom disk tape]

The first one is the system ROMs dir in the user's home directory. The second is the (new) software file pool for other software in the user's home directory. The last two are similar, but then on system level. On a UNIX like system, you get something very similar.

### findcheat

This is a tool to find new cheats, for example for a certain game it can help you find the memory location where the number of remaining lives is stored. These cheats can later be added to the `trainer` command.

It works more or less like this:

1. Initialize the `findcheat` tool (this takes an initial snapshot of the MSX memory)
2. Perform some action in the game that changes the variable that you're interested in. For example if you want to find the memory location where the number of lives is stored, you have to loose (or gain) a life in the game.
3. Now use the `findcheat` tool to compare the current MSX memory state with the previous memory snapshot. `findcheat` offers a lot of possibilities here, for example you can search for memory locations that became bigger or smaller or locations whose value changed or didn't change.
4. `findcheat` will show a list of memory locations that still match the search criteria.
5. If there still are still too many matches, repeat from step 2.

Vampier wrote a very good tutorial on how to use `findcheat`, you can find it here.

### hd<x>

Change the hard disk image. The commands `hda`, `hdb` etc. are assigned to all available hard disk drives in the MSX. They will not correspond to drive names as used in MSX-DOS.

usage:

`hda <disk image>` | Use hard disk image for hard disk "hda"
`hda insert <disk image>` | Use hard disk image for hard disk "hda"
`hda` | Show current hard disk image for hard disk "hda"

Note: Because of disk caching, changing the hard disk when the MSX is running can lead to corruption of the hard disk contents. Therefore openMSX blocks the `hd<x>` commands unless the MSX is powered off. See `power` setting.

### help

Shows help info for console commands.

usage:

`help` | Shows a list of all possible commands
`help <command>` | Shows help info for a specific command
`help <command> <subcommand>` | Some commands have more detailed help on subcommands

### incr

Increment an integer setting.

usage:

`incr <setting>` | Increment the specified setting by one
`incr <setting> <num>` | Increment the specified setting by the given amount

examples:
`incr speed`
`incr renshaturbo 10`
`incr scanline -5`

### iomap

Shows what I/O ports are connected to which devices. The related command `slotmap` shows a similar overview, but for memory-mapped devices.

usage:

`iomap` | Shows the I/O map of the current MSX machine

### keymatrixdown / keymatrixup

Press or release keys in the MSX keyboard matrix. Can be used to make an external program or Tcl script press MSX keys. For some more information about the keymatrix, you could read the article on the MAP.

usage:

`keymatrixdown <row> <mask>` | Press the indicated MSX keys
`keymatrixup <row> <mask>` | Release the indicated MSX keys

examples:
`keymatrixdown 6 0x01`
`keymatrixup 6 0x01`

### laserdiscplayer

Controls the Laserdisc player; a Laserdisc can be inserted or ejected. When a real Laserdisc player is connected to an MSX, no other controls are available either.

Note that this command is only available when the Pioneer PX-7 or Pioneer PX-V60 is being emulated

usage:

`laserdiscplayer insert <filename>` | Inserts the specified file into the virtual laserdisc player.
`laserdiscplayer eject` | Ejects the laserdisc from the virtual laserdisc player; this emulates pressing the eject button on a real Laserdisc Player.

### list_extensions

Returns a list of inserted cartridges and extensions. These can be removed with the `remove_extension` command or additional items can be added with the `cart` and `ext` commands.

usage:

`list_extensions` | Lists all currently inserted cartridges and extensions

### load_icons

Load a different icon set (used for the On Screen Display (OSD) LEDs).

Icon sets are stored in the share/skins directory.

usage:

`load_icons <name>` | Load the given icon set, but don't change the position on the screen.
`load_icons <name> <position>` | Load the given icon set and place them at the requested position. Position can be `bottom`, `top`, `left` or `right`.

### load_settings

Load settings from a given settings XML file. The settings file does not have to be complete: settings that are not mentioned in the given file are left untouched. See also `save_settings`.

usage:

`load_settings <filename>` | Load settings from the given file

### machine

Switch to a new MSX machine.

usage:

`machine` | Returns the handle for the currently active machine
`machine <machine name>` | Switch to the specified machine, also returns the handle for that machine

Note: The machine handle is mostly used by external applications controlling openMSX (see also Controlling openMSX from External Applications). For interactive use you can omit the machine handle to have the commands operate on the current machine.

### create_machine / load_machine / activate_machine / list_machines / delete_machine

openMSX has the possibility to have multiple MSX machines concurrently in memory. This is more or less like multiple tabs in a web browser: you only work with one at-a-time, but you can have multiple open at the same time and easily switch between them. These commands are low level commands to manage this.

Some commands are specific per machine, for example if you insert a disk image into the disk drive of the emulated MSX machine and if you have multiple MSX machines, you need to specify in which MSX machine you want to insert the disk. To solve this, we introduced the concept of the 'active' MSX machine (this is also the machine that is visible and audible). All unqualified machine-specific command will act on the active machine. If you want to execute the command in a specific machine, you can qualify the command with a machineID prefix.

`diska <diskimage>` | execute diska command in the active machine
`<machine-ID>::diska <diskimage>` | execute diska command in the specified machine

#### `create_machine`:

This command returns a new machine-id. This machine-id can be used in the following commands. In the web browser analogy this command would open a new empty tab.

#### `load_machine`:

This command loads a machine configuration (= MSX model) into the given machine-ID. In the web browser analogy, this command would load a page in a previously created empty tab. And unlike a web browser, where you can load a different page in the same tab, you cannot load a different machine configuration in the same machine-ID.

#### `activate_machine`:

This command activates the given machine-ID. At any time there can only be one active machine-ID. This is analogue to switching tabs in a web browser.

#### `list_machines`:

Returns a list of all currently existing machine-IDs.

#### `delete_machine`:

Deletes the given machine-ID. This is analogue to closing a tab in a web browser.

#### examples:

`set oldID [machineID]` | get the current machineID
`set newID [create_machine]` | create a new machineID
`$newID::load_machine Philips_NMS_8250` | load an MSX2 configuration in that new machineID
`activate_machine $newID` | switch to the new machine
`activate_machine $oldID` | switch back to old machine
`delete_machine $newID` | delete new machine

If you don't care about multiple active machines, the `machine` command is much more convenient to switch to a different MSX configuration.

### machine_info

Shows information about a certain topic. This command is similar to the `openmsx_info` command. The topics of `machine_info` are all machine specific, while the topics of `openmsx_info` are generic.

usage:

`machine_info` | Shows a list of all possible topics
`machine_info <topic>` | Shows info on the given topic

### monitor_type

Select a monitor color profile.

usage:

`monitor_type` | Shows the currently selected color profile
`monitor_type -list` | Lists all available color profiles
`monitor_type <profile>` | Selects a new color profile

Note: This command is a convenience wrapper around the `color_matrix` setting.

### mute_channels / unmute_channels / solo

Mute or unmute specific individual channels of sound devices. The syntax is very similar to the `record_channels` command.

usage:

`mute_channels <device> [<channels>]] [<device> [<channels>]]` | Mute the specified channels of the specified device(s). If a device is given but no specific channels are specified, all channels of that device are muted. If no arguments are given at all, this command return a list of all currently muted channels.
`unmute_channels <device> [<channels>]] [<device> [<channels>]]` | Unmute the specified channels of the specified device(s). If a device is given but no specific channels are specified, all channels of that device are unmuted. If no arguments are given at all, this command unmutes all channels of all devices.
`solo <device> [<channels>]] [<device> [<channels>]]` | Mute all channels of all devices except for the specified channels.

examples:
`mute_channels`
`mute_channels PSG`
`mute_channels SCC 2,4`
`unmute_channels`
`unmute_channels PSG 1 SCC 1,3-4`
`solo PSG 3`

### nowind<x>

Similar to the `disk<x>` commands there is a `nowind<x>` command for each nowind interface. This command is modeled after the 'usbhost' command of the real nowind interface. Though only a subset of the options is supported. Here's a short overview of the command line options:

long | short | explanation
--- | --- | ---
--image | -i | specify disk image
--hdimage | -m | specify harddisk image
--romdisk | -j | enable romdisk
--ctrl | -c | no phantom disks
--no-ctrl | -C | enable phantom disks
--allow | -a | allow other diskroms to initialize
--no-allow | -A | don't allow other diskroms to initialize

If you don't pass any arguments to this command, you'll get an overview of the current nowind status.

This command will create a certain amount of drives on the nowind interface and (optionally) insert diskimages in those drives. For each of these drives there will also be a `nowind<x><1..8>` command created. Those commands are similar to e.g. the `diska` command. They can be used to access the more advanced diskimage insertion options.

In some cases it is needed to reboot the MSX before the changes take effect. In those cases you'll get a message that warns about this.

examples:

`nowinda -a image.dsk -j` | Image.dsk is inserted into drive A: and the romdisk will be drive B:. Other diskroms will be able to install drives as well. For example when the MSX has an internal diskdrive, drive C: en D: will be available as well.
`nowinda disk1.dsk disk2.dsk` | The two images will be inserted in A: and B: respectively.
`nowinda -m hdimage.dsk` | Inserts a harddisk image. All available partitions will be mounted as drives.
`nowinda -m hdimage.dsk:1` | Inserts the first partition only.
`nowinda -m hdimage.dsk:2-4` | Inserts the 2nd, 3th and 4th partition as drive A: B: and C:.

### openmsx_info

Shows information about a certain topic. For machine-specific topics, use the related command `machine_info`.

usage:

`openmsx_info` | Shows a list of all possible topics
`openmsx_info <topic>` | Shows info on the given topic

### openmsx_update

Enable or disable update notifications of a certain type. This command is intended for external programs controlling openMSX. More about this in Controlling openMSX from External Applications.

usage:

`openmsx_update enable <type>` | enable notifications for this type
`openmsx_update disable <type>` | disable notifications for this type

examples:
`openmsx_update enable led`
`openmsx_update disable setting`

### osd

openMSX has the possibility to show OSD (on screen display) elements. For example, the LEDs and the fps-indicator are implemented via OSD elements. This command allows to create new OSD elements, configure existing elements or delete elements.

This command is only useful if you plan to adjust or enhance the openMSX OSD, or create your own OSD widgets.

Execute "`help osd`" to get a detailed description of this command, which we will not repeat here.

### palette

Shows the current VDP palette settings. Related command: `vdpregs`.

usage:

`palette` | Show the currently active color palette

### plug / unplug

Plugs or unplugs a plug into a connector, for example plug a virtual joystick into a virtual joystick port.

usage:

`plug` | Shows all currently connected plugs
`plug <connector>` | Shows currently connected plug for the specified connector
`plug <connector> <plug>` | Plugs the specified plug into the specified connector
`unplug <connector>` | Unplugs the plug connected to the specified connector

examples:
`plug cassetteport cassetteplayer`
`plug joyporta mouse`
`plug printerport logger`
`unplug joyportb`

### psg_profile

Select a PSG sound profile.

usage:

`psg_profile` | Shows the currently selected sound profile
`psg_profile -list` | Lists all available sound profiles
`psg_profile <profile>` | Selects a new sound profile

Note: This command is a convenience wrapper around the `PSG_vibrato_frequency`, `PSG_vibrato_percent`, `PSG_detune_frequency` and `PSG_detune_percent` settings.

### record

Controls video recording: write openMSX audio/video to an AVI file.

usage:

`record start` | Record to file "openmsxNNNN.avi"
`record start <filename>` | Record to indicated file
`record start -prefix foo` | Record to file "fooNNNN.avi"
`record stop` | Stop recording
`record toggle` | Toggle recording

The `start` subcommand also accepts an optional `-audioonly`, `-videoonly` and a `-doublesize` flag. Videos are recorded in a 320×240 size by default and at 640×480 when the `-doublesize` flag is used. If only audio is recorded, the created file will be a WAV file instead of an AVI file.

If any stereo sound devices are present or any sound device has an off-center balance, the recording will be made in stereo, otherwise it will be mono. If a recording is made in mono and then a stereo sound device is added, you'll receive a warning that stereo sound has been detected and that the two channels will be mixed down to mono. You can prevent this from happening by using the `-stereo` option to force a stereo recording even if no stereo devices are present at the time you enter the command. You can also force a mono recording with `-mono` to save space.

The `soundlog` command is a shorthand for `record -audioonly`.

Use `record_chunks` if you want some extra options. You can control the maximum length (in seconds) to record and also set up multiple recordings of a certain length. This is very useful if you want to record for e.g. YouTube. The default length is 14:59 (to make sure YouTube will accept it). Using this command implies `-doublesize`.

### record_channels

A high level command to record individual channels of sound chips to separate files. In the following variants of the command you can specify devices and channels. Multiple devices can be specified and multiple channels as well. If you want to specify channels of a device, put them right after the device. You can also specify `all` for the device, which means that all sound devices in the currently running MSX will be recorded. When starting recording, an option `-prefix` can be given to specify a filename prefix.

usage:

`record_channels [start] <device> [<channels>] [<device> [<channels>]] [-prefix <prefix>]` | Start recording the specified channel(s) of the specified device(s). If no channels are given, all channels of the device are recorded.
`record_channels stop [<device> [<channels>]] [<device> [<channels>]]` | Stop recording the specified channel(s) of the specified device(s). If no channels are given, recording for all channels is stopped for the given device(s). If no devices are given, all channel recording is stopped.
`record_channels all -prefix justtesting` | Record all channels of all sound devices and create the file names with prefix 'justtesting' (e.g. to quickly delete all these files again).
`record_channels list` | Lists which channels of which sound chips are currently being recorded.

examples:
`record_channels start PSG`
`record_channels PSG`
`record_channels SCC 1,4-5`
`record_channels SCC PSG 1`
`record_channels "MSX Music" 7-9 SCC 3,5 PSG 2`
`record_channels stop`
`record_channels stop PSG`
`record_channels stop SCC 3,5`
`record_channels list`

### remove_extension

Remove a cartridge or extension from a running MSX machine. See also the commands `cart`, `ext`, `list_extensions`.

usage:

`remove_extension fmpac` | Removes the FMPAC extension from the running MSX

### reset

Emulates the pressing of the reset button on the MSX. This sends a reset pulse to all devices, but does not erase memory contents.

usage:

`reset` | Resets the current machine

### reverse

Controls the reverse feature. When this feature is enabled (the default), openMSX will collect data while emulating, which enables you to go back (and forward) in MSX time. In other words: you cannot use the commands to go back and forward in time, if you disable the feature.

usage:

`reverse start` | Start collecting data (enable the reverse feature).
`reverse stop` | Stop collecting data (disable reverse feature) and remove all collected data.
`reverse status` | Gives information about the reverse feature and the data it collected. Mostly useful for scripts.
`reverse goback <n>` | Go back <n> seconds in time. Of course, you cannot go back to a time before the time the `reverse start` command was given.
`reverse viewonlymode <on|off>` | Control the view only mode of the reverse feature. In view only mode, the replay will never get interrupted by any user actions that normally would interrupt the replay. Use this to safely view a replay without accidentally ruining it by touching a key.
`reverse goto <time>` | Go to the indicated absolute moment in MSX time (given in seconds). If the time is before the time openMSX started collecting data (with the `reverse start` command) openMSX will jump to the time when collecting started.
`reverse savereplay [<filename>]` | Save the collected data (an initial savestate and all collected input events) to a file.
`reverse loadreplay [-goto <begin|end|savetime|<n>>] [-viewonly] <filename>` | Load the replay from the given file and start it. Loads the initial snapshot and starts replaying the recorded events. Enables the reverse feature automatically. With the `-goto` option, you can specify where to jump to in the replay after loading (`begin` is default), where `savetime` is the time at which the replay was saved and `n` is an absolute time in seconds in the replay. The `-viewonly` option is a shortcut to put the reverse feature in viewonly mode directly after loading the replay. Without this option, it will always go to normal mode.

There are some extra helper commands to make the feature easier to use.

usage:

`go_back_one_second` / `go_forward_one_second` | Go back or forward one second in time (if possible). These are used for the default PageUp and PageDown key bindings.
`reverse_prev [<min> [<max>]]` | Go back in time to the previous (internal) snapshot. The further back in the past the less dense the amount of snapshots are. So, executing this command multiple times, will take successively bigger steps in the past. You can optionally specify a minimal and maximal step size. You will at least go back the minimal amount of time (even if there's a snapshot closer to the current time) and at most the maximal amount of time (even if there's no snapshot within the maximum specified time from the current time).
`reverse_next [<min> [<max>]]` | As `reverse_prev` but then it goes to the closest snapshot in the future (if possible).

Because the reverse feature is very useful, it is automatically enabled via `auto_enable_reverse` setting.

### save_settings

Write the current openMSX settings to a settings XML file. See also `load_settings`.

If you disabled `save_settings_on_exit`, you can use this command to save your preferences.

usage:

`save_settings` | Save settings to the default settings file
`save_settings <filename>` | Save settings to the given file

### savestate / loadstate / list_savestates / delete_savestate

These command can be used to manage savestates. These are much easier to use than the lowlevel `store_machine` and `restore_machine` commands.

#### `savestate [<name>]`

This creates a snapshot of the currently emulated MSX machine. Optionally you can specify a name for the savestate, if you omit this name, the default name `quicksave` will be taken.

#### `loadstate [<name>]`

This restores a previously created savestate. Like above you can specify a name which defaults to `quicksave` if omitted.

#### `list_savestates`

This returns the names of all previously created savestates.

#### `delete_savestate <name>`

Delete a previously created savestate.

### screenshot

Take a screenshot of the openMSX screen. By default this takes a screenshot of the 'scaled' MSX screen (see `scale_algorithm` setting) without OSD elements (e.g. console and icons). If you want to include the OSD elements pass the `-with-osd` option. If you want a screenshot of the 'unscaled' raw MSX screen, pass the `-raw` option. The screenshots are PNG files and (by default) are saved in the `screenshots` subdirectory of the openMSX data directory in your home directory. There's also an option `-no-sprites` to take a screenshot with sprite rendering disabled.

usage:

`screenshot [-with-osd] [-raw [-doublesize]] [-no-sprites] [-prefix <prefix>] [<filename>]`

examples:

`screenshot` | Write screenshot to file "openmsxNNNN.png"
`screenshot <filename>` | Write screenshot to indicated file
`screenshot -prefix foo` | Write screenshot to file "fooNNNN.png"
`screenshot -raw` | Create screenshot of the raw MSX screen only (so no icons or console and no scaling)
`screenshot -raw -doublesize` | Create screenshot of the raw MSX screen only, with resolution 640×480
`screenshot -with-osd` | Create screenshot of the scaled screen, including OSD elements
`screenshot -no-sprites` | Create screenshot with sprite rendering disabled

### set

Change or query the value of various settings. See also: `unset`.

usage:

`set <setting>` | Query the current value of the specified setting
`set <setting> <value>` | Change the specified setting to the given value

The settings that can be adjusted with this command are listed and explained at the end of this document.

examples:
`set accuracy pixel`
`set blur 25`
`set scanline 20`
`set deinterlace on`

### slotmap

Shows what devices are inserted into which slots. The related command `iomap` shows a similar overview, but for I/O mapped devices.

usage:

`slotmap` | Shows the slot map of the current MSX machine

### slotselect

Shows the currently selected slots. To see what devices are located in the slots, use the `slotmap` command.

usage:

`slotselect` | Shows the currently selected slot for each page

### soundlog

Controls sound logging: writing the openMSX sound to a WAV file.

This command is a shorthand for `record -audioonly`.

usage:

`soundlog start` | Log sound to file "openmsxNNNN.wav"
`soundlog start <filename>` | Log sound to indicated file
`soundlog start -prefix foo` | Log sound to file "fooNNNN.wav"
`soundlog stop` | Stop logging sound
`soundlog toggle` | Toggle sound logging state

### store_machine / restore_machine

These are low-level commands, used to implement savestates.

#### `store_machine`:

Saves the state of the specified machine to a file.

`store_machine` | Save state of current machine to file "openmsxNNNN.xml.gz"
`store_machine <machineID>` | Save state of indicated machine to file "openmsxNNNN.xml.gz"
`store_machine <machineID> <filename>` | Save state of indicated machine to specified file

#### `restore_machine`:

Load a previously saved machine in a new machine-ID, next to the already available machines. See the section on `activate_machine`.

`restore_machine` | Load state from last saved state in default directory
`restore_machine <filename>` | Load state from indicated file

Note: These commands are pretty low level. The `savestate` and `loadstate` scripts are built on top of this and are much more convenient to use.

### test_machine

Test whether the given MSX machine configuration works. For example whether you have all required system-roms for this machine. See also `load_machine`.

usage:

`test_machine <machine-config>` | Test whether the given machine configuration is OK.

### toggle

Toggles any boolean (on/off) setting: if it was on, it will be turned off and vice versa.

usage:

`toggle <setting>` | Toggles the specified setting

examples:
`toggle mute`
`toggle throttle`

### trainer

Control game trainers. You can enable or disable individual cheats of each trainer. Make use of the TAB key to see what is available. When switching trainers, the currently active trainer will be deactivated.

usage:

`trainer` | See which trainer is currently active
`trainer <game>` | See which cheats are currently active in the trainer
`trainer <game> all` | Activate all cheats in the trainer of <game>
`trainer <game> \[<cheat> ..\]` | Toggle cheats of <game> on/off
`trainer deactivate` | Deactivate all trainers

examples:
`trainer Frogger all`
`trainer "Circus Charlie" 1 2`
`trainer Pippols lives "jump shoes"`

### type

Type a string in the emulated MSX. This command automatically presses and releases keys in the simulated MSX keyboard matrix. This command is useful for demoing and for automating tasks in MSX-BASIC.

usage:

`type "Hello world!"` | Yet another manifestation of the most famous program

### unset

Undefines a Tcl variable. When used on openMSX settings, they are reverted to their default value. See also: `set`.

usage:

`unset <variable>` | Undefines the given variable
`unset <setting>` | Reverts the given setting to its default value

### user_setting

This command is only meant to be used in Tcl scripts. It allows to create Tcl variables that act very much like built-in openMSX settings. They have a description (can be queried with "`help set <setting-name>`") and their value is stored saved/restored when openMSX is quit/restarted.

Execute "`help user_setting`" to get a detailed description of this command.

### vdpregs

Shows the current register settings of the Video Display Processor (VDP). Related command: `palette`.

usage:

`vdpregs` | Shows the current VDP control register contents

### other

Most commands described above are generally useful. openMSX also has a bunch of other more specialized commands. Some of these are intended for programmers who code MSX programs using openMSX as a tool. Other of these commands are more like toys or examples that show the openMSX scripting capabilities.

We've only listed a very brief overview of these command. As always execute "`help <command-name>`" to get a more detailed description of the command.

`about` | Search command help-texts for given keyword
`cpuregs` | Gives overview of the CPU registers
`data_file` | Helps locate openMSX data files
`disasm` | Print disassembled instructions at given memory location
`getcolor` | Query V99x8 palette settings
`get_active_cpu` | Returns the active cpu, z80 or r800
`get_color_count` | Gives an overview of the used colors in the current screen
`get_screen` | Capture the content of a MSX text screen in a Tcl string
`get_screen_mode` | Decodes the current screen mode from the VDP registers and returns it as a Tcl string. `get_screen_mode_number` returns it as a number which would also be used for the basic command `SCREEN`.
`get_selected_slot` | Returns the selected slot for the given memory page
`guess_title` | Use heuristics to guess the title of the current game (cartridge, disk or tape). For specific media use `guess_cassette_title`, `guess_disk_title` or `guess_rom_title`.
`listing` | Reimplementation of the BASIC LIST command in Tcl
`load_debuggable` | Write the content of a file to a openMSX debuggable
`main_menu_open` / `main_menu_close` / `main_menu_toggle` | Control the visibility of the default OSD menu
`multi_screenshot` | Take screenshots of multiple successive frames
`pc_in_slot` | Check whether CPU is executing from the specified slot (useful as breakpoint condition)
`peek` | Read a byte from given memory location
`peek16` | Read a 16 bit word from given memory location
`poke` | Write a byte to given memory location. Use `dpoke` to only write if the to be written value is different than the current value.
`poke16` | Write a 16 bit word to given memory location
`psg_log` | Log or replay PSG register values in binary format
`ram_watch` | Add or remove RAM watch addresses to/from the list on the right side of the screen, useful for debugging or TASing
`reg` | Read or write CPU registers
`reg_log` | Log or replay register values for the specified debuggable in ASCII format
`rom_info` | Gives information about the given ROM device, coming from the software database. If no argument is given, the first found (external) ROM device is assumed. This command replaces the info that was previously (before openMSX 0.8.1) automatically printed on stdout.
`run_to` | Execute instructions until PC reaches specified address
`save_debuggable` | Save the content of a debuggable to a file
`setcolor` | Change V99x8 palette settings
`set_help_text` | Associate help text with a Tcl proc
`set_tabcompletion_proc` | Associate tab completion with a Tcl proc
`showdebuggable` | Print the content of a debuggable in a table
`showmem` | Print the content of memory in a table
`show_osd` | Print an overview of the defined OSD elements
`skip_instruction` | Skip the current CPU instruction
`sprite_viewer` | Show a widget with which you can view the sprite patterns
`stack` | Print the top of the CPU stack
`step_in` | Execute one CPU instruction, go into subroutines
`step_over` | Execute one CPU instruction, but don't go into subroutines
`step_out` | Step out of the current subroutine
`step_back` | Step one instruction back in time
`text_echo` | Echo all printed MSX text on stderr
`toggle_cursors` | Show (or hide) a widget which shows which keys are pressed
`toggle_fps` | Show (or hide) an fps indicator
`toggle_frame_counter` | Show (or hide) a widget which shows the current frame number since start-up
`toggle_freq` | Switch between PAL/NTSC
`toggle_info_panel` | Show (or hide) a panel with various types of info on the currently running MSX (emulation); similar to the info in the panel you get when using the DIGIblue theme in blueMSX
`toggle_mog_overlay` | Enable (or disable) graphical extra information and game hints when playing The Maze of Galious
`toggle_mog_editor` | Enable (or disable) wall drawing and Popolon-placement with the mouse when playing The Maze of Galious; needs to have the MoG overlay enabled, see `toggle_mog_overlay`
`toggle_music_keyboard` | Enable (or disable) keyboard view of all existing music channels. EXPERIMENTAL! Be careful, it's very slow when many channels are present in the system
`toggle_nemesis_1_shield` | Enable (or disable) an OSD drawn shield in Nemesis (Gradius) 1, all enemy objects will repel from it
`toggle_osd_keyboard` | Show (or hide) an on-screen keyboard (mostly useful for devices without physical keyboard); only supports an international layout for now
`toggle_psg2scc` | Enable (or disable) playing PSG sound on SCC
`toggle_reversebar` | Show (or hide) the reverse bar, which helps to control and view the data of the reverse feature, which is automatically enabled when the bar is enabled
`toggle_scc_editor` | Show a graphical view of the SCC chip(s) of the system, showing waveforms and volume per channel and also enables you to edit the waveforms per channel
`toggle_scc_viewer` | Show a graphical view of the SCC chip(s) of the system, showing waveforms and volume per channel
`toggle_show_palette` | Show (or hide) a graphical view on the palette registers
`toggle_vdp_access_test` | Enable (or disable) reporting in the console when VDP I/O is done which could possibly cause data corruption on the slowest VDP (TMS9xxx), which is not emulated
`toggle_vdp_reg_viewer` | Enable (or disable) a widget that shows an overview of all VDP registers and highlights changes in the values
`toggle_vu_meters` | Show (or hide) a graphical view of the volumes of the sound channels of several sound chips
`umrcallback` | Example proc to use with the umr_callback setting
`vdpcmdinprogresscallback` | Example proc to use with the vdpcmdinprogress_callback setting
`v9990reg` | Read or write a V9990 register
`v9990regs` | Print an overview of all V9990 registers
`vdpreg` | Read or write a V99x8 register
`vdrive` | Easily switch disks in multi-disk games
`vpeek/vpoke` | Read/write bytes from/to video RAM

The source code of all these scripts is located in `share/scripts` directory. Feel free to inspect these scripts and modify them to suit your needs.

## Old Commands

The following commands existed in older openMSX versions. For backwards compatibility they are still supported for a while. In later versions they will be removed.

### alias / unalias

Create a new command that is an alias for another (group of) command(s).

It is better to use the more powerful Tcl `proc` command.

usage:

`alias <name> <command>` | Defines an alias

examples:
`alias gl "set renderer SDLGL-PP"`
`alias restart "set power off ; set power on"`
Note: The backwards compatibility implementation of the `alias` command is not 100% compatible with the old `alias` command. It is recommended that you update your scripts to use the Tcl `proc` command.

### decr

Decrement an integer setting.

This command is deprecated, please use the `incr` command with a negative offset instead.

usage:

`decr <setting>` | Decrement the specified setting by one
`decr <setting> <num>` | Decrement the specified setting by the given amount

examples:
`decr speed`
`decr renshaturbo 10`

### quit

Quits the emulator.

Please use `exit` instead.

usage:

`quit` | Exits openMSX

### restoredefault

Restore the default value for a setting.

This command is deprecated, please use `unset <setting>` instead.

usage:

`restoredefault <setting>` | Restores the default value for the given setting

examples:
`restoredefault PSG_volume`

## Settings

Settings control many aspects of openMSX. Below, the available settings are listed and described. You can change setting values with the `set` command.

### accuracy

Sets the render accuracy. openMSX supports three levels of render accuracy:

screen accurate:
  Changes in VDP state become effective only once per video frame. Works well for most MSX1 software, but will break a lot of MSX2 software (anything that does so-called raster effects).
line accurate:
  Changes in VDP state become effective only once per display line. Works well for almost all software.
pixel accurate:
  Changes in VDP state become effective immediately. In this mode even the 'Unknown Reality scope part' is rendered correctly.

In some cases switching to a lower accuracy level can speed up emulation, but in many cases the speed difference is negligible.

The default is pixel accuracy, since this is the most realistic. If the software you are running shows a jittery screen split and you would prefer a stable screen split, switching to line accuracy can help.

usage:

`set accuracy` | Shows the current setting
`set accuracy screen` | Selects screen accurate rendering
`set accuracy line` | Selects line accurate rendering
`set accuracy pixel` | Selects pixel accurate rendering

### audio-inputfilename

Sets the audio file from which the wave input is read for the sampler.

By default, it is read from "audio-input.wav" when available.

usage:

`set audio-inputfilename` | Shows the current setting
`set audio-inputfilename mysample.wav` | Read from "mysample.wav"

Note: The file is fully read into memory, so under Linux/UNIX do not attempt to read from a device node such as `/dev/dsp`.

### autoruncassettes

Switches the "auto-run cassettes" feature on or off. When it's enabled, openMSX will try to type the proper loading instruction when a cassette is inserted.

usage:

`set autoruncassettes` | Shows the current setting
`set autoruncassettes on` | Try to run cassettes automatically
`set autoruncassettes off` | Do nothing when cassettes are inserted

Note: This only works with CAS images for now and it is still an experimental feature.

### autorunlaserdisc

Switches the "auto-run laserdisc" feature on or off. When it's enabled, openMSX will try to type the proper loading instruction when a laserdisc is inserted.

usage:

`set autorunlaserdisc` | Shows the current setting
`set autorunlaserdisc on` | Try to load Laserdiscs automatically
`set autorunlaserdisc off` | Do nothing when Laserdiscs are inserted

### auto_enable_reverse

Using the `reverse` feature has a small memory and performance cost. Therefore it has to be enabled before it can be used. This setting controls whether the reverse feature should automatically be activated when openMSX starts. On desktop computers this generally won't be a problem. But for small handheld devices it can be.

usage:

`set auto_enable_reverse` | Shows the current setting
`set auto_enable_reverse off` | Don't automatically enable the reverse feature
`set auto_enable_reverse on` | Enable the reverse feature when openMSX starts
`set auto_enable_reverse gui` | Enable the reverse feature and the reverse bar when openMSX starts

### blur

Sets the amount of horizontal blur effect. A value of 0 turns off blur, while 100 selects maximum blur.

usage:

`set blur` | Shows the current setting
`set blur <value>` | Change the value

Note: Only some scale algorithms apply horizontal blur; the default algorithm "simple" does.

### bootsector

Sets the boot sector type for DirAsDSK. Default: DOS2. Only relevant on turboR, because it boots differently depending on the type of boot sector on the disk in drive A.

usage:

`set bootsector` | Shows the current setting
`set bootsector DOS1` | Use a DOS1 boot sector

### brightness

Controls the brightness of the video output. Can be between -100 and 100. Lower values are darker, higher values are brighter. The default is 0, which is neutral. This setting shifts the brightness of all colors, including black and white, while the `gamma` setting changes the relative brightness of colors but does not change black and white.

The section about the `noise` setting describes a typical way of using `brightness`.

usage:

`set brightness` | Shows the current setting
`set brightness 5` | Make the video output a bit brighter than default

### cmdtiming

Controls VDP command execution timing.

This is useful for debugging and for speeding up games where the command engine performance is a bottleneck.

usage:

`set cmdtiming` | Shows the current setting
`set cmdtiming broken` | Make VDP commands finish instantly
`set cmdtiming real` | Make VDP commands take a realistic amount of time

Note: When set to `broken` the emulated MSX acts different from a real MSX. This might cause some software to fail.

### color_matrix

This setting represents a 3×3 matrix that is used to transform MSX RGB colors to host RGB colors. This setting can be used to generate all kind of color schemes, see `scripts/monitor.tcl` for examples.

To get the following color transformation:

            | a b c |   | Rm |   | Rh |
            | d e f | × | Gm | = | Gh |
            | g h i |   | Bm |   | Bh |

Use this command:

            set color_matrix { { a b c } { d e f } { g h i } }

usage:

`set color_matrix` | Shows the current value
`set color_matrix { { 1 0 0 } { 0 1 0 } { 0 0 1 } }` | This is the default (no color transformation)
`set color_matrix { { .33 .33 .33 } { .33 .33 .33 } { .33 .33 .33 } }` | Transform to grey scale

Note: It is often more convenient to use the `monitor_type` command.

### console

Turns the openMSX on-screen console on or off.

usage:

`set console` | Shows the current setting
`set console on` | Turns the console on
`set console off` | Turns the console off

### consolebackground

Change the console background image. Only images in the PNG format are supported. Background images may also have an alpha channel (amount of transparency per pixel).

usage:

`set consolebackground` | Shows the current setting
`set consolebackground <image>` | Sets a new background image

### consolecolumns

Change the width of the console measured by the number of columns.

usage:

`set consolecolumns` | Shows the current setting
`set consolecolumns <value>` | Set the specified width

### consolefont

Change the console font. This should be the filename of a True Type Font. The default value is `skins/VeraMono.ttf.gz`.

In older openMSX releases (pre-0.7.1). You had to specify a PNG image here that contained a 16×16 matrix with the characters in ASCII order. This is no longer supported.

usage:

`set consolefont` | Shows the current setting
`set consolefont <myfont.ttf>` | Sets a new font

### consolefontsize

Set the size for the console font. The default value is 12.

usage:

`set consolefontsize` | Shows the current setting
`set consolefont 16` | Set a bigger than default font size

### console_history_size

Determines how many commands are saved into the console history.

usage:

`set console_history_size` | Shows the current setting
`set console_history_size 5000` | Keep a maximum of 5000 commands in the console history

### consoleplacement

Changes the position of the console on the emulator screen.

usage:

`set consoleplacement` | Shows the current setting
`set consoleplacement <place>` | Moves the console to the specified location; `<place>` can be `topleft`, `top`, `topright`, `left`, `center`, `right`, `bottomleft`, `bottom` or `bottomright`.

### consolerows

Change the height of the console measured by the number of rows.

usage:

`set consolerows` | Shows the current setting
`set consolerows <value>` | Set the specified width

### console_remove_doubles

Determines whether the console history remembers two identical subsequent commands.

usage:

`set console_remove_doubles` | Shows the current setting
`set console_remove_doubles on` | Remove (do not remember) the last command if it's the same as the previous (default)
`set console_remove_doubles off` | Allow double subsequent command entries in the console history

### contrast

Controls the contrast of the video output. Can be between -100 and 100. Lower values are less contrast, higher values are more contrast. The default is 0, which is neutral.

The section about the `noise` setting describes a typical way of using `contrast`.

usage:

`set contrast` | Shows the current setting
`set contrast -5` | Reduce the video contrast a bit

### cputrace

Enable/disable CPU instruction tracing. When enabled, the state of the CPU (Z80/R800) is printed on stdout after every instruction. This creates a lot of output and slows down emulation considerably, but it can be very useful for debugging.

usage:

`set cputrace` | Shows the current setting
`set cputrace on` | Enables CPU tracing
`set cputrace off` | Disables CPU tracing

### debugoutput

Selects the file to where the output from the debug device goes.

The User's Manual describes the debug device in more detail.

usage:

`set debugoutput` | Shows the current output file name
`set debugoutput stdout` | Writes debug output to openMSX's standard output stream
`set debugoutput stderr` | Writes debug output to openMSX's standard error stream
`set debugoutput <output file>` | Writes debug output to the specified file

Note: This setting only exists if the `debugdevice` extension is present in the current MSX machine.

### default_machine

Selects the default MSX model. openMSX uses this machine when it is started without the `-machine` option. This is a typical setting that should be saved, see also `save_settings`.

usage:

`set default_machine` | Shows current setting
`set default_machine Panasonic_FS-A1GT` | Use the turboR GT the next time openMSX is started

### DirAsDSKmode

Determine the behavior of the DirAsDSK when inserting a directory to be used as diskimage.

The possible values are `read_only`, `cached_write`, `nodelete` and `full`.

Although it is the most risky mode, the default is set to `full`, since this is what most users expect from using DirAsDSK.

`read_only` | The MSX can not write to the virtual disk. Changes on the host-OS are still reflected on the virtual disk, however.
`cached_write` | The MSX can write to the virtual disk, however, all changes are only cached in memory, no changes are passed onto the host-OS. Changes on the host-OS are still reflected on the virtual disk and will override any changes that the MSX has made.
`nodelete` | Changes are two ways, from host-OS to MSX and vice versa. However, deleting a file on the MSX will not delete the file on the host-OS. This can lead to unexpected behavior when the MSX later recreates a file with the same name, since this will be reflected towards the host-OS.
`full` | All changes are performed both ways, no restrictions apply.

usage:

`set DirAsDSKmode` | Shows the current setting
`set DirAsDSKmode read_only` | Disk image will be read only

Note: this setting is only used when the directory is inserted, it is not possible to change the behaviour of the current virtual disk by altering the setting. The new setting will become effective after the current virtual disk has been ejected.
Note: On turboR machines, the MSX keeps a cache of the directory sectors in memory. This means that changes made on the host OS are detected by the DirAsDSK routine, but will not show up in those machines. The data sectors will have been changed when reading, however. This can cause unexpected data to be read in the MSX environment. To rectify this situation, perform a disk eject and reinsert the directory again. This will cause the hardware switch that the turboR has to be toggled, and its internal cache to be invalidated. Since the turboR machines do not use a write cache, the changes on the MSX side are correctly written to the host OS.

### deinterlace

Turns deinterlacing on/off. Deinterlace is a filter which combines the even and odd field of interlaced video into a single frame which has double vertical resolution. It results in a sharp and stable image, but can show artifacts on fast animations.

usage:

`set deinterlace` | Shows the current setting
`set deinterlace on` | Turns deinterlacing on
`set deinterlace off` | Turns deinterlacing off

Note: Deinterlacing is only supported for `scale_factors` bigger or equal to 2.

### disablesprites

Can be used to disable sprite rendering. Only the rendering itself is disabled, all other MSX behaviour (like sprite collision detection) stays the same.

usage:

`set disablesprites` | Shows the current setting
`set disablesprites on` | Disable sprite rendering
`set disablesprites off` | Enable sprite rendering (the default)

### display_deform

Select display deformation effect. This effect is only supported in the SDLGL-PP renderer.

usage:

`set display_deform` | Shows the current setting
`set display_deform normal` | Turns off display deform
`set display_deform 3d` | Deforms the image in 3D, to look like a CRT (like JEmu2)

Note: In the past there was also a 'horizontal_stretch' mode. This is now replaced by the `horizontal_stretch` setting.

### enable_session_management

Controls session management. When enabled, openMSX will store the state of all machines when you exit openMSX and restore that state again when starting it up next time. Note that the reverse history is not saved.

Sessions can also be saved manually with the command `save_session`, and explicitly loaded with `load_session`. A list of saved sessions can be retrieved with `list_sessions`.

### frequency

Sets the sound mixer frequency. Sound hardware and sound APIs typically support a limited set of frequencies, such as 11025 Hz, 22050 Hz, 44100 Hz and 48000 Hz.

usage:

`set frequency` | Shows the current setting
`set frequency 44100` | Use 44.1 kHz mixing frequency (CD quality)

### firmwareswitch

Some machines (e.g. turboR) have a switch on the front (or on the back) that controls if the machine should boot 'normally' or start the built-in software, also called firmware. This setting controls the position of that switch.

usage:

`set firmwareswitch` | Shows the current setting
`set firmwareswitch on` | Boot into the internal software
`set firmwareswitch off` | Boot into MSX-BASIC or on-disk software

### fullscreen

Switch to/from fullscreen mode.

usage:

`set fullscreen` | Shows the current setting
`set fullscreen on` | Switch to fullscreen mode
`set fullscreen off` | Switch to windowed mode

### fullspeedwhenloading

When enabled, openMSX will try to detect when the MSX is loading from diskette, cassette or laserdisc. During loading openMSX will run at full speed (`throttle` off). This can be convenient if you're not interested in the realistic but slow loading times on MSX. Default is off, because it is not according to the behaviour of a real MSX.

Unlike the fast loading features in for example fMSX, `fullspeedwhenloading` does not intercept BIOS calls. Instead, it speeds up the emulation of the entire MSX, including all hardware devices.

usage:

`set fullspeedwhenloading` | Shows the current setting
`set fullspeedwhenloading on` | Load as fast as possible
`set fullspeedwhenloading off` | Load at the same speed as a real MSX

### gamma

Sets the amount of gamma correction. A value of 1.0 will turn off gamma correction. Lower values will result in a darker image, higher values in a brighter image.

If you want to get a realistic picture, set the openMSX gamma correction to PC gamma / MSX gamma. TVs use a standardised gamma of 2.5, let's take that as the value of MSX gamma. You can measure the gamma of your PC screen with a simple test such as the Gamma Measurement Image in Robert W. Berger's "An Explanation of Monitor Gamma". If your PC gamma would be for example 2.0, the most realistic value for gamma correction would be 2.0 / 2.5 = 0.8.

Alternatively, you can just try a few values and see what you like.

usage:

`set gamma` | Shows the current value
`set gamma <num>` | Sets a new gamma correction amount

### glow

Sets the amount of afterglow effect: 0 is off and 100 is a very heavy afterglow.

usage:

`set glow` | Shows the current setting
`set glow <value>` | Change the amount of afterglow

Note: Not all renderers support this.

### grabinput

Controls whether openMSX grabs all input events or not. When this setting is turned on, all input events are directly passed to openMSX. The mouse pointer can't leave the openMSX window and the window manager won't be able to react to keyboard shortcuts.

You can turn this setting on when you want to use mouse-controlled MSX software while openMSX is in windowed mode. It is best turned off in all other cases. See also `escape_grab`.

usage:

`set grabinput` | Shows the current setting
`set grabinput on` | Starts grabbing all input events
`set grabinput off` | Stops grabbing all input events

### horizontal_stretch

Sets the amount of horizontal stretch, thus also the aspect ratio of the screen. More specifically, a setting of `n` means stretch the center `n` MSX pixels to the full width of the host output window (at `scale_factor` 1).

usage:

`set horizontal_stretch` | Shows the current setting
`set horizontal_stretch <value>` | Change the amount of horizontal stretch

examples of typical useful values:
`set horizontal_stretch 320` (no horizontal stretch)
`set horizontal_stretch 272` (approach real aspect ratio of MSX screen)
`set horizontal_stretch 280` (default: show all generated border pixels, so that all border demo effects are still visible)
`set horizontal_stretch 256` (borders are not visible at all; doesn't work well in combination with set-adjust)
Note: when using the SDL renderer, this setting may cause a lot more CPU usage (e.g. on a Dingoo) when not using 320.

### inputdelay

Input events for the MSX machine are delayed by this amount. Increase this value when the MSX machine misses keyboard presses when you type very fast. Decrease this value to reduce the latency between pressing a key on the host machine and seeing it being typed in the MSX machine.

usage:

`set inputdelay` | Shows the current value
`set inputdelay <time>` | Sets the input delay to the specified number of seconds

Note: The default value of 0.03 seconds should almost always be OK, this small delay is practically not noticeable and still allows the MSX machine to get accurate timing on the input events. Please do not change the value of this setting unless you know what you are doing.

### kbd_auto_toggle_code_kana_lock

Switches the "Automatically toggle the CODE/KANA lock" feature on or off. When it's on, openMSX will automatically toggle the CODE/KANA lock when a user enters a character for which the CODE/KANA lock state must be changed.

usage:

`set kbd_auto_toggle_code_kana_lock` | Shows the current setting
`set kbd_auto_toggle_code_kana_lock on` | Automatically toggle the CODE/KANA lock when required
`set kbd_auto_toggle_code_kana_lock off` | Only toggle CODE/KANA lock status when user presses the CODE/KANA lock key

Note: This only works on MSX models for which the CODE/KANA key locks (e.g. Japanese MSX models and the Philips VG8010). On other models, this setting is ignored.

### kbd_code_kana_host_key

Host key that maps to the MSX CODE/KANA key.

It is especially useful for people with AZERTY host keyboard, on which the right-ALT key (RALT, which is the default value of this setting) has a special function; it is called the ALT-GR key and it's used to enter some special characters (some keys are tagged with 3 characters; normal, key+SHIFT, key+ALT-GR).

It is also useful for people with a Japanese (jp106) keyboard; they can map the HENKAN_MODE key (which is similar to the KANA Lock on Japanese MSX models) to the CODE/KANA key.

usage:

`set kbd_code_kana_host_key` | Shows the current setting
`set kbd_code_kana_host_key MENU` | Binds the MENU key on the host keyboard to the MSX CODE/KANA key
`set kbd_code_kana_host_key HENKAN_MODE` | Binds the HENKAN_MODE key on the host keyboard to the MSX CODE/KANA key

### kbd_mapping_mode

The keyboard driver can work in two mapping modes; KEY mapping and CHARACTER mapping.

KEY mapping:
  A key pressed on the host keyboard maps to one specific key on the MSX keyboard. This mode is convenient when the host keyboard and the MSX keyboard have the same layout or when working with a program that directly reads the keyboard matrix and forces the user to enter a certain key combination that can not be auto-generated in the CHARACTER mapping mode.
CHARACTER mapping:
  A character entered by the user is mapped to the correct key combination on the MSX to enter that character. For example, when the user enters an ! character and openMSX is emulating an 'international' MSX model, the keyboard driver will press SHIFT and 1 on the MSX keyboard. This will be done regardless of the key or keys that the user pressed on the host keyboard to enter the ! character.
  This is especially useful when the user has an AZERTY host keyboard and is working on a QWERTY style MSX or when he has a US-QWERTY keyboard and is working on a Japanese MSX.
  Note that special keys (like CAPSLOCK) are mapped directly, just like in the KEY mapping mode.

usage:

`set kbd_mapping_mode` | Shows the current mode
`set kbd_mapping_mode CHARACTER` | Set the CHARACTER mapping mode
`set kbd_mapping_mode KEY` | Set the KEY mapping mode

### kbd_numkeypad_always_enabled

Some real MSX computers do not have a numeric keypad. openMSX will ignore key presses on the host numeric keypad when emulating such an MSX model. With this parameter, you can indicate that even on such MSX models, presses on the host numeric keypad must be mapped to the MSX numeric keypad. So, you can override accurate behaviour with it, which is the reason that by default, this setting is set to 'off'.

usage:

`set kbd_numkeypad_always_enabled` | Shows the current setting
`set kbd_numkeypad_always_enabled on` | Enables numeric keypad, even if the emulated MSX does not have one

### kbd_numkeypad_enter_key

There is a subtle difference between numeric keypad of MSX computers and of most host computers; the MSX computers have a '.' and a ',' on the numeric keypad. On the other hand, the host computers have a '.' and an 'ENTER' key on the keypad.

In some respect it is logical that the 'ENTER' key on the host numeric keypad is mapped to the 'normal' MSX 'ENTER' key. On the other hand, that would make it impossible to enter the ',' on the MSX numeric keypad. Therefore, the user can choose whether the host numeric keypad ENTER key should be mapped to the MSX numeric keypad ',' (which is the default) or to the main 'ENTER' key.

usage:

`set kbd_numkeypad_enter_key` | Shows the current value
`set kbd_numkeypad_enter_key ENTER` | Maps the keypad enter key to the main 'ENTER' key, instead of the comma key on the MSX keypad

### kbd_trace_key_presses

Log SDL key code, SDL modifiers and Unicode value for each key that gets pressed on the host keyboard on stderr. Also show Unicode value and corresponding MSX key-presses for characters that get 'pasted' into the MSX by the console `type` command. This setting is especially useful when defining unicode keymap files, so that you can find out the unicode values belonging to certain keys/characters.

usage:

`set kbd_trace_key_presses` | Shows the current setting
`set kbd_trace_key_presses on` | Turn logging of key presses on

### keyjoystick<n>.<button>

Configure the keys of the keyjoysticks. It's likely this will change in the future.

Valid values for `<n>`: `1`, `2`.

Valid values for `<button>`: `up`, `down`, `left`, `right`, `triga`, `trigb`.

usage:

`set keyjoystick1.up W`
`set keyjoystick1.down S`
`set keyjoystick1.left A`
`set keyjoystick1.right D`
`set keyjoystick1.triga SPACE`

### led_<name>

These are read-only settings. Their value reflects the current status of the corresponding LED on the emulated MSX machine. The currently supported LED names are: `power`, `caps`, `kana`, `pause`, `turbo` and `FDD`.

As for any setting you can use the native `trace` Tcl command to trigger a callback when the value of these settings changes. (In fact this possibility was the main motivation to make these read-only settings instead of topics of the `machine_info` command.)

### limitsprites

Controls whether the VDP has a limit on the number of sprites it can display per line. The default is on, because the real VDP has such a limit. You can turn off the limit to reduce sprite flashing in games such as Aleste. Note that some games (Penguin Adventure, among others) make use of this limitation, so they will display incorrectly if the limit is turned off.

The 5th/9th sprite status flag of the VDP is not influenced by the `limitsprites` setting: the flag always takes the limit into account.

usage:

`set limitsprites` | Shows the current value
`set limitsprites on` | Limits number of sprites per line
`set limitsprites off` | Turns off number of sprites per line limit

### master_volume

Controls the overall openMSX volume. The volume of individual sound devices can be controlled with the `<soundchip>_volume` settings.

usage:

`set master_volume` | Shows current setting
`set master_volume 50` | Sets master volume to 50%

### maxframeskip

Sets the maximum amount of frames to skip: show a frame and then skip at most <number> frames. So 0 means show everything (no frame skipping), 1 means show at least every second frame etc.

Frame skipping is done on demand, as a way to keep the flow of time for the emulated MSX in sync with the flow of real time. You can set limits on the amount of frame skipping with the `minframeskip` and `maxframeskip` setting.

In a situation where the number of consecutive frames specified by `maxframeskip` has been skipped, openMSX will display the next frame, even if that means emulation will start lagging behind real time.

When `throttle` is off, the number of skipped frames will be equal to `maxframeskip`.

usage:

`set maxframeskip` | Shows the current setting
`set maxframeskip <number>` | Sets the maximum number of consecutive frame skips

### midi-in-readfilename

Sets the file from which the MIDI input is read. By default, it is set to `/dev/midi` when available.

usage:

`set midi-in-readfilename` | Shows the current setting
`set midi-in-readfilename mymidilog.dat` | Read MIDI events from "mymidilog.dat"

### midi-out-logfilename

Sets the file to which the MIDI output is logged. By default, it logs to `/dev/midi` when available.

usage:

`set midi-out-logfilename` | Shows the current setting
`set midi-out-logfilename mymidilog.dat` | Log MIDI events to "mymidilog.dat"

### minframeskip

Sets the minimum amount of frames to skip: show a frame and then skip at least <number> frames. So 0 means no forced frame skipping, 1 means skip at least every second frame etc.

Frame skipping is done on demand, as a way to keep the flow of time for the emulated MSX in sync with the flow of real time. You can set limits on the amount of frame skipping with the `minframeskip` and `maxframeskip` setting.

The `minframeskip` setting can be useful if you want to ease the burden on your PC processor, for example for longer battery life on a laptop. It can also be useful if your PC is consistently too slow to run without frame skipping: in such cases video might be smoother with a low but constant frame rate than with a fluctuating frame rate.

usage:

`set minframeskip` | Shows the current setting
`set minframeskip <number>` | Sets the number of frame skips

### mode

Sets the active mode. A mode is a set of settings (mostly key bindings, but also OSD widgets that are activated) that are most suitable for a certain task. Currently only mode 'normal' and 'tas' exist.

usage:

`set mode` | Shows the current setting
`set mode tas` | Change mode to TAS mode
`set mode normal` | Set mode back to normal, which is the default (all purpose) mode

#### TAS mode

So far, the only special mode is the TAS mode, which is made for doing Tool Assisted Speedruns, with TAS widgets and easier ways to save replays. It is still experimental, but already very useful for doing a TAS. This mode enables the following widgets:

- frame counter (can also be toggled with `toggle_frame_counter`), which shows the VDP (not V9990) frame number on screen
- cursors (can also be toggled with `toggle_cursors`), shows which keys (important for games) are pressed

It also (re)enables the reverse bar widget.

The mode configures the following key bindings, overriding any existing key bindings (note: Mac key bindings are not proper yet...):

keys (PC) | keys (Mac) | function
--- | --- | ---
F6 | (F6) | Load replay from current slot
F7 | (F7) | Open slot select menu
F8 | (F8) | Save replay to current slot
End | (End) | Advance one frame (`advance_frame`)
ScrollLock | (ScrollLock) | Reverse one frame (`reverse_frame`)

Note that this mode is still experimental and may change in future releases!

### mute

Mute/unmute all sound output.

usage:

`set mute` | Shows the current setting
`set mute on` | Mute sound
`set mute off` | Unmute sound

### noise

Controls the amount of Gaussian noise that is added to the video output. A small amount of noise can give a more authentic look to the video output on TFTs. Values can be between 0 and 100, where 0 is no noise and 100 is lots of noise.

This setting is best combined with `brightness` and `contrast`: noise creates small random fluctuations in the brightness of pixels. When noise is applied to pure black, it is not possible to make it any darker, so half of the time the noise is ineffective. The same happens with pure white. By setting the `brightness` slightly above 0 and `contrast` slightly below 0, you will get a better looking noise effect.

usage:

`set noise` | Shows the current setting
`set noise 7` | Add a moderate amount of noise

### pause

Pauses the emulation.

usage:

`set pause` | Shows the current setting
`set pause on` | Pauses emulation
`set pause off` | Unpauses emulation

Note: Some video settings cannot be applied to an already rendered frame and will therefore not take effect until openMSX is unpaused.

### pause_on_lost_focus

When this setting is enabled, the emulation will be paused when the openMSX window loses focus.

usage:

`set pause_on_lost_focus` | Shows the current setting
`set pause_on_lost_focus on` | Emulation will be paused when the openMSX window loses focus
`set pause_on_lost_focus off` | Emulation will continue when the openMSX window loses focus (default)

### pointer_hide_delay

The amount of seconds before the mouse pointer will be automatically hidden after it got shown due to mouse activity. A negative amount means that it will never be hidden, an amount of 0 means that it will be always hidden. By default the pointer is hidden 1 second after the last mouse activity.

usage:

`set pointer_hide_delay` | Shows the current setting
`set pointer_hide_delay -1` | Never hide the mouse pointer
`set pointer_hide_delay 0` | Always hide the mouse pointer
`set pointer_hide_delay 3.4` | Hide the mouse pointer after 3.4 seconds of inactivity

### power

Turn the power of the emulated MSX machine on or off.

usage:

`set power` | Shows the current setting
`set power on` | Turns the MSX machine on (the default)
`set power off` | Turns the MSX machine off

### printerlogfilename

Sets the file to which the printer logger writes.

usage:

`set printerlogfilename` | Shows the current setting
`set printerlogfilename myprinterlog.txt` | Log to "myprinterlog.txt"

### print-resolution

Sets the resolution (in dpi) for the emulated dot-matrix printer.

The emulated printer 'prints' pages as PNG files. This settings determines the resolution of those images.

usage:

`set print-resolution` | Shows the current setting
`set print-resolution 600` | Sets resolution to 600 dpi

### r800_freq / r800_freq_locked

These two settings control the R800 clock frequency. See `z80_freq / z80_freq_locked` for details.

### renderer

Switch to a different video renderer. See the User's Manual for a description of the available renderers.

usage:

`set renderer` | Shows the current setting
`set renderer <name>` | Switches to the given renderer

### renshaturbo

Sets the speed of the built-in auto fire on some Japanese MSX models, for example the turboR machines. A value of 0 turns off auto fire, while 100 selects the most rapid auto fire.

usage:

`set renshaturbo` | Shows the current renshaturbo value
`set renshaturbo <num>` | Sets speed to value <num>

Note: This setting is only available if the current MSX machine has hardware Rensha Turbo support.

### resampler

Sets the method to resample the sound of sound chips from their native frequency to the desired output frequency.

usage:

`set resampler` | Shows the currently active resampler
`set resampler fast` | Sets a fast, but low quality resampler. This uses simple linear interpolation, which can result in very audible aliasing effects in some cases. Although this is a relatively low quality algorithm, it's the algorithm that was used in pre-0.6.3 openMSX versions (and most other MSX emulators).
`set resampler blip` | Sets the Blip_Buffer based resampler, which has the best quality per CPU usage ratio (this is the default value).
`set resampler hq` | Sets the highest quality resampler, but it also takes the most CPU time. It's based on the libsamplerate algorithm.

### rs232-inputfilename

Sets the file from which the RS232-tester reads data. Note that the `rs232-tester` has to be plugged in the `msx-rs232` connector for this to become useful. When plugging the tester, this setting needs to point to a valid file.

usage:

`set rs232-inputfilename` | Shows the current setting
`set rs232-inputfilename myrs232input.txt` | Reads from "myrs232input.txt"

### rs232-outputfilename

Sets the file to which the RS232-tester writes the data. Note that the `rs232-tester` has to be plugged in the `msx-rs232` connector for this to become useful. When plugging the tester, this setting needs to point to a valid file.

usage:

`set rs232-outputfilename` | Shows the current setting
`set rs232-outputfilename myrs232output.txt` | Write to "myrs232output.txt"

### rtcmode

Sets the Real Time Clock mode. Can be either `RealTime` or `EmuTime`.

In `RealTime` mode the MSX clock is always synchronized with the host clock, even when for example emulation is paused for a while or when emulation is run at 200% of real speed.

In `EmuTime` mode the time is only synchronized with the host clock when openMSX starts. From then on the clock ticks at the same pace as the emulated machine. So when emulation is paused, the clock is paused as well. If emulation is run at 200% speed, the clock also ticks twice as fast.

In `EmuTime` mode it's not possible for a MSX program to detect whether it's running on a real or on an emulated machine. That's why this is the default mode. On the other hand the `RealTime` mode might be better if for example you care that timestamps of files written by the emulated MSX machine are in sync with the host machine time.

usage:

`set rtcmode` | Shows the current mode
`set rtcmode EmuTime` | Set EmuTime mode (the default)
`set rtcmode RealTime` | Set RealTime mode

### samples

Sets the size of the sound mixer buffer. Higher values help against buffer underruns (hickups), but increase the latency of the sound output.

usage:

`set samples` | Shows the current setting
`set samples 1024` | Use a mixing buffer of 1024 samples

### save_settings_on_exit

Automatically save the current settings when openMSX exits: execute a `save_settings` command on exit.

usage:

`set save_settings_on_exit` | Show current setting
`set save_settings_on_exit on` | Enable auto save
`set save_settings_on_exit off` | Disable auto save

### scale_algorithm

Selects the algorithm used to transform MSX pixels to host pixels. The User's Manual contains more information about scalers.

usage:

`set scale_algorithm` | Shows the current setting
`set scale_algorithm simple` | Selects the default scale algorithm
`set scale_algorithm hq` | Selects the HQ2x/3x/4x scale algorithm

Note: Not all renderers support all scale algorithms.

### scale_factor

Selects the scale factor. Scale factor <n> means the typical MSX pixel (MSX resolution 256×212) is mapped on <n> by <n> host pixels. For the moment the possible values are 1 to 4. In the future we may support a wider range or even non-integer values. The User's Manual contains more information about scalers.

usage:

`set scale_factor` | Shows the current setting
`set scale_factor <n>` | Sets a new scale factor

Note: Not all renderers support all scale factors.

### scanline

Sets the amount of scanline effect.

usage:

`set scanline` | Shows the current setting
`set scanline <value>` | Changes the value

Note: Some scalers will not render scanlines at all.

### sound_driver

Select the sound output driver. The list of available sound drivers is platform specific.

usage:

`set sound_driver sdl` | Selects the SDL sound driver (all platforms)
`set sound_driver directx` | Selects the DirectX sound driver (Windows only)

### speed

Sets the emulation speed relative to the speed of a real MSX. Speed 100 means as fast as a real MSX, lower values are slower than real MSX, higher values are faster than real MSX.

usage:

`set speed` | Shows current emulation speed
`set speed <num>` | Sets new emulation speed

### <soundchip>_balance

Sets the balance (distribution over the left and right channel) for individual sound chips. It replaces the previously available `<soundchip>_mode` setting. The range is between -100 (totally left) and 100 (totally right).

usage:

`set <soundchip>_balance` | Shows the current setting
`set <soundchip>_balance 0` | Plays the output of this chip on both the left and right channel
`set <soundchip>_balance -100` | Plays the output of this chip on only the left channel
`set <soundchip>_balance 75` | Plays the output of this chip mostly on the right channel, but also a bit on the left channel

examples:
`set PSG_balance`
`set PSG_balance -100`
`set FMPAC_balance 0`

### <soundchip>_ch<channel>_record

Sets the filename to which the sound of an individual channel of individual sound chips should be recorded. When this setting is not set, no recording takes place and recording starts as soon as the setting is set. Normally, you would probably prefer to use the `record_channels` command to set up channel recording instead of this low level setting.

usage:

`set <soundchip>_ch<channel>_record` | Shows the current setting
`set <soundchip>_ch<channel>_record filename` | Starts recording the sound of the specified chip and channel to the file with name <filename>

examples:
`set SCC_ch1_record`
`set PSG_ch3_record /tmp/PSG_ch3.wav`

### <soundchip>_ch<channel>_mute

Use to mute a specific channel of an individual sound chip. Normally, you would probably prefer to use the `mute_channels` command to set up channel muting instead of this low level setting.

usage:

`set <soundchip>_ch<channel>_mute` | Shows the current setting
`set <soundchip>_ch<channel>_record on` | Mutes the sound of the specified channel of the specified chip
`set <soundchip>_ch<channel>_record off` | Unmutes the sound of the specified channel of the specified chip

examples:
`set SCC_ch1_mute`
`set PSG_ch3_mute on`
`set SCC_ch5_mute off`

### <soundchip>_detune_frequency

Sets the frequency of the detune (a random variation in a sound's frequency) effect. It makes a sound fatter and more natural, as if played by a human being.

usage:

`set <soundchip>_detune_frequency` | Shows the current setting
`set <soundchip>_detune_frequency <num>` | Sets new detune frequency in Hz; 1 is minimum, 100 is maximum

examples:
`set PSG_detune_frequency`
`set PSG_detune_frequency 5` (default)
Note: For now, this setting is only available for the PSG soundchip.
Note: It is often more convenient to use the `psg_profile` command.

### <soundchip>_detune_percent

Sets the strength of the detune effect. By default it is 0, which means the effect is switched off.

usage:

`set <soundchip>_detune_percent` | Shows the current setting
`set <soundchip>_detune_percent <num>` | Sets new detune strength; 0 is minimum, 10 is maximum

examples:
`set PSG_detune_percent`
`set PSG_detune_percent 0` (switched off, default)
`set PSG_detune_percent 0.5` (recommended)
Note: For now, this setting is only available for the PSG soundchip.
Note: It is often more convenient to use the `psg_profile` command.

### <soundchip>_vibrato_frequency

Sets the frequency of the vibrato (a periodic variation in a sound's frequency) effect.

usage:

`set <soundchip>_vibrato_frequency` | Shows the current setting
`set <soundchip>_vibrato_frequency <num>` | Sets new vibrato frequency in Hz; 1 is minimum, 10 is maximum

examples:
`set PSG_vibrato_frequency`
`set PSG_vibrato_frequency 5` (default)
Note: For now, this setting is only available for the PSG soundchip.
Note: It is often more convenient to use the `psg_profile` command.

### <soundchip>_vibrato_percent

Sets the strength of the vibrato effect. By default it is 0, which means the effect is switched off.

usage:

`set <soundchip>_vibrato_percent` | Shows the current setting
`set <soundchip>_vibrato_percent <num>` | Sets new vibrato strength; 0 is minimum, 10 is maximum

examples:
`set PSG_vibrato_percent`
`set PSG_vibrato_percent 0` (switched off, default)
`set PSG_vibrato_percent 1` (recommended)
Note: For now, this setting is only available for the PSG soundchip.
Note: It is often more convenient to use the `psg_profile` command.

### <soundchip>_volume

Sets the volume for individual sound chips. The overall volume is controlled by the `master_volume` setting.

usage:

`set <soundchip>_volume` | Shows the current setting
`set <soundchip>_volume <num>` | Sets new volume; 0 is off, 100 is maximum

examples:
`set PSG_volume`
`set PSG_volume 60`
`set "FMPAC_volume" 50`

### throttle

Sets throttle mode. In throttle mode the emulator tries to run at the specified speed relative to a real MSX (see speed command). When throttling is turned off the emulator runs as fast as possible.

usage:

`set throttle` | Shows the current setting
`set throttle on` | Turn throttle mode on (normal operation)
`set throttle off` | Turn throttle mode off (fast forward)

### turborpause

Controls the pause key on a MSX turboR machine.

usage:

`set turborpause` | Shows the current setting
`set turborpause on` | Activate the pause key
`set turborpause off` | Deactivate the pause key

Note: If you use this setting often, it may be useful to bind it to a key on your PC keyboard. See the `bind` and `toggle` commands.

### umr_callback

Selects the Tcl procedure to be called when an Uninitialized Memory Read has been detected. This is useful for debugging MSX programs: uninitialized memory is not guaranteed to have any particular value, so reading it is most likely a bug.

By default this setting is empty, which means that nothing is done when an Uninitialized Memory Read is detected. We ship a useful procedure called `umrcallback` which logs all UMRs. You can activate it with `set umr_callback umrcallback`. You can find the source code for this procedure in `scripts/umrcallback.tcl`.

usage:

`set umr_callback` | Shows the current UMR callback setting
`set umr_callback umrcallback` | Sets callback proc to `umrcallback`

### vdpcmdinprogress_callback

Selects the Tcl procedure to be called when a write to a VDP command engine register is detected while there is still a VDP command in progress. Often this is an indication of a bug in the running MSX program. Note that writes to VDP register R#44 with a command in progress are normal behaviour, so the callback is not triggered for such writes.

By default this setting is empty, which means that nothing is done when a suspicious VDP command engine write is detected. We ship an example proc called `vdpcmdinprogresscallback` which simply logs all occurrences. You can activate it with `set vdpcmdinprogress_callback vdpcmdinprogresscallback`. You can find the source code for this proc in `scripts/umrcallback.tcl`. Feel free to write your own proc that does exactly what you need. For example it might be a good idea to execute `debug break` in your callback, so that you can easily examine what code triggered this write.

usage:

`set vdpcmdinprogress_callback` | Shows the current value. Default is "" (meaning no action)
`set vdpcmdinprogress_callback vdpcmdinprogresscallback` | Sets callback to `vdpcmdinprogresscallback`

### vdpcmdtrace

Enable/disable VDP command tracing. When enabled, every VDP command is logged on stdout. This is useful when debugging MSX programs that use the VDP command engine.

usage:

`set vdpcmdtrace` | Shows the current setting
`set vdpcmdtrace on` | Enables VDP command tracing
`set vdpcmdtrace off` | Disables VDP command tracing

### videosource

Switch between `MSX` (V99x8) or `GFX9000` (V9990) video source.

usage:

`set videosource` | Shows the current setting
`set videosource MSX` | Switch to normal MSX screen
`set videosource GFX9000` | Switch to GFX9000 screen

Note: This setting is only available if the `gfx9000` extension is present.

### v9990cmdtrace

Enable/disable V9990 command tracing. This is the V9990 equivalent of `vdpcmdtrace`.

usage:

`set v9990cmdtrace` | Shows the current setting
`set v9990cmdtrace on` | Enables V9990 command tracing
`set v9990cmdtrace off` | Disables V9990 command tracing

Note: This setting is only available if the `gfx9000` extension is present.

### z80_freq / z80_freq_locked

These two settings control the Z80 clock frequency. When `z80_freq_locked` is true the emulated Z80 runs at the normal 3.5 MHz (or optionally 5.3 MHz on some machines). When `z80_freq_locked` is false the value of `z80_freq` is taken as the Z80 clock frequency.

examples:
Overclock Z80 to 14 MHz:
`set z80_freq 14318180`
`set z80_freq_locked false`
F8 switches between 3.5 MHz and 7 MHz:
`set Z80_freq 7159090`
`bind F8 "toggle z80_freq_locked"`

$Id: commands.html 12343 2012-01-07 11:51:03Z m9710797 $