This directory contains a so-called "Boosted" MSX2+ configuration. It has the
following features:

- based on Panasonic FS-A1WSX (most complete MSX2+), which includes:
  - Kanji ROM
  - MSX-MUSIC
  - firmware
- three external slots, slot B and C are in a sub slot (2-1 and 2-3)
- 2048 kB memory mapper (in slot 3-0)
- 2 disk drives
- V9958 VDP with 192 kB VRAM
- SCC+ in slot 2-0
- MSX Audio
- MoonSound with 640 kB sample RAM
- GFX9000
- 512 kB MegaRAM in slot 2-2
- BASIC Compiler (MSX-BASIC Kun)

This configuration needs the following ROMs:
- fs-a1wsx_kanjifont.rom, fs-a1wsx_basic-bios2p.rom, fs-a1wsx_fmbasic.rom,
  fs-a1wsx_msx2psub.rom, fs-a1wsx_kanjibasic.rom, fs-a1wsx_disk.rom,
  fs-a1wsx_firmware.rom: same as needed for the Panasonic FS-A1WSX machine
- phc-70fd2_basickun.rom: same as needed for the basic compiler in the Sanyo
  PHC-70FD2
- yrw801.rom: same as needed for the MoonSound extension

You can make this configuration the default by changing the 'default_machine'
setting from the console. See the Setup Guide and User's Manual sections of the
manual.
